	ESS Spiking Pump & Weigh Scale Inventory, Operational Status, Planned Upgrades & Dedicated Usages

	Type Pump/

Manu/

Model No.
	Pump

Serial #


	ESS

Equip #
	Motor

Size,

HP
	Max Cap,

GPH
	Max Disc. Press

(Press Gage, Max)

Press. Relief Setting,

PSI
	Mat’ls of

Construc-

tion1
	Liq Only

or Both

Liq &

 Disp’s.
	FB-

Control

Capab’ly.

?

	I. Diaphragm-Type, Positive-Displacement, Metering Pumps

	A. LMI

	C-111-75HV
	010411796
	LMI#1
	NA
	2.5
	150
	PP,T,SS
	Both
	No

	C-111-75HV
	010411797
	LMI#2
	NA
	2.5
	150
	PP,T,SS
	Both
	No

	E-511-75HV(EP)
	931101075
	LMI#3
	NA
	2.5
	150  (400,200)  150
	PP,T,SS
	Both
	Yes

	C-911-75HV
	980312990
	LMI#4
	NA
	2.5
	150  (200)  150
	PP,T,SS
	Both
	Yes

	C-761-75-HPP
	0303746809-1
	LMI#5
	NA
	4.0
	175  (800,200)  175
	PP,T,SS
	Both
	Yes

	C-761-75-HPP
	0307774891-1
	LMI#6
	NA
	4.0
	175  (400,200)  175
	PP,T,SS
	Both
	Yes

	C-761-75-HPP
	0308785695-2
	LMI#7
	NA
	4.0
	175 (200)  175
	PP,T,SS
	Both
	Yes

	C-761-75-HPP
	0308785695-3
	LMI#8
	NA
	4.0
	175  (300,200)  175
	PP,T,SS
	Both
	Yes

	E-761-75-HPP(EP)
	-
	LMI#9
	NA
	4.0
	175  (200)  175
	PP,T,SS
	Both
	Yes

	E-761-75-HPP(EP)
	-
	LMI#10
	NA
	4.0
	175  (200)  175
	PP,T,SS
	Both
	Yes

	B. Neptune4

	532-A-N3-FA-EX1(EP)
	106718
	Nept#3
	0.25
	11.0
	350  (1,000,400)  350
	V,T,SS
	Liquids
	Yes

	535-A-N3-FA-EX1(EP)
	100581
	Nept#4
	0.25
	18.0
	350  (300,400)  350
	V,T,SS
	Liquids
	Yes

	535-VS-N3
	126047
	Nept#5
	0.33
	18.0
	300  (400)  300
	V,T,SS
	Both
	Yes

	535-VS-N3
	126048
	Nept#6
	0.33
	18.0
	300  (1,000,400)  300
	V,T,SS
	Both
	Yes

	547-VS-N3-FA-T17
	145485
	Nept#7
	0.75
	30.0
	500  (1000,600)  500
	V,T,SS
	Both
	Yes

	547-VS-N3-FA-T17
	145486
	Nept#8
	0.75
	30.0
	500  (1000,600)  500
	V,T,SS
	Both
	Yes

	547-VS-N3-FA-E17
	148694
	Nept#9
	0.75
	30.0
	500  (600)  500
	V,T,SS
	Both
	Yes

	547-VS-N3-FA-E17
	148695
	Nept#10
	0.75
	30.0
	500  (600)  500
	V,T,SS
	Both
	Yes

	567-A-N3-FA-E17
	101291
	Nept#11
	0.75
	80.0
	250  (1000,300)  250
	V,T,SS
	Liquids
	Yes

	C. Wilden

	M-1
	NA
	Wil#1
	Air
	600.0
	150  (200)  150
	T,SS
	Liquids
	Yes

	M-1
	NA
	Wil#2
	Air
	600.0
	150  (200)  150
	T,SS
	Liquids
	Yes

	II. Progressive-Cavity-Type, Positive-Displacement, Transfer Pumps

	A. Moyno5

	33101
	WJ
	Moy#1
	0.5
	1052
	150  (300,200)  150
	B or V, CI
	Both
	Yes

	33101
	WJ
	Moy#2
	0.5
	1052
	150  (300,200)  150
	B or V, CI
	Both
	Yes

	33101(EP)
	NA
	Moy#3
	0.75
	1052
	150  (300,200)  150
	B or V, CI
	Both
	Yes

	33101(EP)
	NA
	Moy#4
	0.75
	1052
	150  (300,200)  150
	B or V, CI
	Both
	Yes

	33301
	NA
	Moy#5
	
	3002
	502
	B or V, CI
	Both
	Yes

	B. Continental

	CP22-C5FMT
	CP10577
	Cont#1
	
	1702
	1002
	B or V, CI
	Both
	Yes

	Pump Related Footnotes:

	1. Materials of Construction:
	Legend: ( = Planned Purchases
	2. Pump Capacity vs. Pressure Head Curves:

	A.   B=
	Buna Rubber
	( = Fitted for FB Control
	Model No
	GPH
	@
	Head, PSI

	B.   CI=
	Cast Iron
	( = Requires Maintenance &/or Revised Equip/Settings
	33101
	120
	@
	0

	C.   PP=
	Polypropylene
	( = Designated Spare &/or Not Skid Mounted
	
	105
	@
	75

	D.   SS=
	Stainless Steel
	( = Designated as a Dispersion Only Pump
	
	90
	@
	150

	E.   T=
	Teflon
	( = Explosion Proof (EP) &/or Intrinsically Safe (IS) Equip
	33301
	570
	@
	0

	F.   V=
	Viton
	
	
	435
	@
	25

	
	4. All Neptune pumps have internal pressure relief/recycle.
	
	300
	@
	50

	
	Additionally, all ESS pump skids are equipped with 
	CP22-
	300
	@
	0

	
	external pressure relief valves.  To the extent practical, both
	C5FMT
	210
	@
	50

	
	will be set @ the same pressure.
	
	120
	@
	100

	Weigh Scales:
	Weight Standards: Certified Annually w Traceability to NIST Standards. Certified 9/2003.

	Field (F1–F6):
	6 Units, 1,000 Lbs + 0.05 - 0.1 Lbs.(IS)
	Field:
	25 - 50.00 Lbs Standards (ESS#1 - #25)

	Shop/Spare(S1-S2):
	2 Units, 1,000 Lbs + 0.05 - 0.1 Lbs.(IS)
	Lab/Shop:
	  1 - 25.00 Lbs Standard (ESS#26)

	Lab  (L1):
	1 Unit, 300 Lbs + 0.015 - 0.03 Lbs.
	Lab:
	One (32 Piece, 51+ Lbs) Set of SS Laboratory Weight Standards (Lbs):

	(L2):
	1 Unit, 50 Lbs + 0.0025 - 0.005 Lbs.
	
	(a)  3-10,

(b)  3-5,

(c)  5-1,

(d)  1-0.5,

(e)  1-0.25,
	(f)  2-0.2,

(g) 1-0.125,

(h) 1-0.1,

(i)  1-0.0625,

(j)  1-0.05
	(k)  1-0.03125,

(l)   2-0.02

(m) 1-0.015625,

(n)  1-0.01,

(o)  1-0.0078125,
	(p) 1-0.005,

(q) 1-0.00390625,

(r)  2-0.002,

(s) 2-0.00195125, &

(t)  1-0.001.

	(L3):
	1 Unit, 15 Lbs + 0.00075 - 0.0015 Lbs.
	
	
	
	
	

	(L4):
	1 Unit, 1 Lb + 0.00001 to 0.00002 Lb.
	
	
	
	
	

	5 Moyno Stators Available in Buna for Dispersions & solutions, & Viton  for MCB, Perc, Etc.  All Seals/Flex Joints Are in Viton.
	
	
	
	
	

	6 Five (5) Neptune pumps equipped w EP Motors & Stoke Controllers.  Three additional EP enclosures/cables sets are available for installation where needed.


(Rev #14, 1/30/2004
